Infonique

iSEB Expansion Board 1200 0012 V1.2

|  |  |  |
| --- | --- | --- |
| Prepared by | Date | Version |
| Bing Ran | 06/10/2023 | 1.2 |

# Abstract

This document provides detailed of Infonique iSEB Expansion Board 1200 0012 V1.1 specification.

# Document History

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Rev** | **Modifier** | **Changes** |
| **15-July-2023** | 1.0 | Bing Ran | First Draft |
| **10-Sept-2023** | 1.1 | Bing Ran | Further elaboratoin about WiFi and servo motor |
| **06-Oct-2023** | 1.2 | Bing Ran | Further elaboratoin & update naming |
|  |  |  |  |
|  |  |  |  |

# Contents

[Abstract 2](#__RefHeading___Toc1131_1720759766)

[Document History 2](#__RefHeading___Toc1133_1720759766)

[Contents 3](#__RefHeading___Toc1135_1720759766)

[1 Introduction 6](#__RefHeading___Toc1141_1720759766)

[2 Hardware 7](#__RefHeading___Toc450_3933630546)

[2.1 Schematic 7](#__RefHeading___Toc452_3933630546)

[2.2 Pinout 8](#__RefHeading___Toc1042_1019879922)

[2.2 PCB Layout 9](#__RefHeading___Toc456_3933630546)

[2.2.1 Label of legs 10](#__RefHeading___Toc458_3933630546)

[2.2.2 PWM control 11](#__RefHeading___Toc460_3933630546)

[2.2.2.1 PWM Control Servo Motor Connection 11](#__RefHeading___Toc2710_4244800993)

[2.2.3 Battery Connector & RGB Led 13](#__RefHeading___Toc1044_1019879922)

[2.2.4 Switch 14](#__RefHeading___Toc1046_1019879922)

[2.2.5 MT3608 step-up converter 15](#__RefHeading___Toc2712_4244800993)

[2.2.5 Buzzer 16](#__RefHeading___Toc2714_4244800993)

[2.2.6 TP4056 module 17](#__RefHeading___Toc2716_4244800993)

[2.2.7 Capacitor and resistor 18](#__RefHeading___Toc2718_4244800993)

[2.3 Bom list 18](#__RefHeading___Toc2720_4244800993)

[3 Firmware 19](#__RefHeading___Toc464_3933630546)

[3.1 Specification of the ESP32 DevKit V1 19](#__RefHeading___Toc1048_1019879922)

[3.2 Environment set up 20](#__RefHeading___Toc1050_1019879922)

[3.3 WiFi 24](#__RefHeading___Toc996_1617206542)

[3.3.1 How the WiFi Code works 24](#__RefHeading___Toc1010_1617206542)

[3.3.2 WiFi server and control UI 25](#__RefHeading___Toc1052_1019879922)

[3.4 Servo Motor 30](#__RefHeading___Toc998_1617206542)

[3.4.1 How the Servo Motor Code works 31](#__RefHeading___Toc1000_1617206542)

[3.4.1.1 Setup 31](#__RefHeading___Toc1002_1617206542)

[3.4.1.2 Code of motorInit function 32](#__RefHeading___Toc1002_1617206542_Copy_1)

[3.4.1.3 Update duty cycle during runtime 33](#__RefHeading___Toc1004_1617206542)

[3.4.1.4 Set\_PWM\_to\_Servo 33](#__RefHeading___Toc1021_1617206542)

Table of Figures

[Figure 1: Robot that controlled by iSEB Expansion Board 1200 0012 V1.0. 6](#Figure!0|sequence)

[Figure 2: Schemaitc of iSEB Expansion Board 1200 0012 V1.2 7](#Figure!1|sequence)

[Figure 3: iSEB Expansion Board 1200 0012 V1.0 without ESP32 Module 9](#Figure!2|sequence)

[Figure 4: iSEB Expansion Board 1200 0012 V1.0 with ESP32 Module 9](#Figure!3|sequence)

[Figure 5: Classification of Walking and Merus legs 10](#Figure!4|sequence)

[Figure 6: PWM control port 11](#Figure!5|sequence)

[Figure 7: SMLab iCrab’s Merus legs 12](#Figure!6|sequence)

[Figure 8: SMLab iCrab’s Walking legs 12](#Figure!7|sequence)

[Figure 9: Battery connector & RGB led 13](#Figure!8|sequence)

[Figure 10: Battery Switch 14](#Figure!9|sequence)

[Figure 11: MT3608 Step-up Converter circuit 15](#Figure!10|sequence)

[Figure 12: Schematic of MT3608 step up converter 15](#Figure!11|sequence)

[Figure 13: Buzzer 16](#Figure!12|sequence)

[Figure 14: TP4056 Module 17](#Figure!16|sequence)

[Figure 15: Capacitor and resistor 18](#Figure!13|sequence)

[Figure 16: Pinout of ESP32 DevKit V1 19](#Figure!14|sequence)

[Figure 17: File -> Preferences and click on the icon 20](#Figure!17|sequence)

[Figure 18: Adding board manager URLS 20](#Figure!18|sequence)

[Figure 19: Install ESp32 by Espressif Systems at Board Managers 21](#Figure!19|sequence)

[Figure 20: Instal WS2812FX library 21](#Figure!20|sequence)

[Figure 21: Upload setting 22](#Figure!21|sequence)

[Figure 22: Compile and upload 23](#Figure!22|sequence)

[Figure 23: WiFi List 25](#Figure!23|sequence)

[Figure 24: Access ISEB Crab through web broswer 25](#Figure!24|sequence)

[Figure 25: Control Page 26](#Figure!25|sequence)

[Figure 26: Motion Editor Page 27](#Figure!26|sequence)

[Figure 27: Zero Page 28](#Figure!27|sequence)

[Figure 28: setting page 29](#Figure!28|sequence)

[Figure 29: How servo’s position controlled by PWM signal 30](#Figure!15|sequence)


Index of Tables


[Table 1: Pinout 7](#Table!0|sequence)

[Table 2: Position vs GPIO vs Channel vs Connector matrix 31](#Table!1|sequence)

# 1 Introduction

This document will discuss the details of the iSEB Expansion Board 1200 0012 V1.0. iSEB Expansion Board 1200 0012 V1.0 is design for a SMLab iCrab robot. It provide 8 rgb leds (red green blue leds ) and 16 pwm output to control the servo motors. The following figure is one of the robot that control with iSEB Expansion Board 1200 0012 V1.0.



Figure 1: Robot that controlled by iSEB Expansion Board 1200 0012 V1.0.

# 2 Hardware

## 2.1 Schematic




Figure 2: Schemaitc of iSEB Expansion Board 1200 0012 V1.2

## 2.2 Pinout

|  |  |  |  |
| --- | --- | --- | --- |
| **Pin** | **Function** | **Pin** | **Function** |
| EN | Enable Pin | D23 | PWM16 |
| VP | Unused | D22 | Unused |
| VN | Unused | TX0 | TX0 |
| D34 | Unused | RX0 | RX0 |
| D35 | ADC Vbatt | D21 | RGB Led |
| D32 | PWM8 | D19 | PWM15 |
| D33 | PWM7 | D18 | PWM14 |
| D25 | PWM6 | D05 | PWM13 |
| D26 | PWM5 | D17 | PWM12 |
| D27 | PWM4 | D16 | PWM11 |
| D14 | PWM3 | D04 | PWM10 |
| D12 | PWM2 | D02 | Buzzer |
| D13 | PWM1 | D15 | PWM9 |

Table 1: Pinout

## 2.2 PCB Layout

The following is the figure of the iSEB Expansion Board 1200 0012 V1.0




Figure 3: iSEB Expansion Board 1200 0012 V1.0 without ESP32 Module




Figure 4: iSEB Expansion Board 1200 0012 V1.0 with ESP32 Module

### 2.2.1 Label of legs

The following figure is labeling the legs of the SMLab iCrab.

Figure 5: Classification of Walking and Merus legs

## 

### 2.2.2 PWM control

There are 16 PWM control port in iSEB Expansion Board 1200 0012 V1.0. The figure below is showing the locaiton of the 16 PWM control port.






Figure 6: PWM control port


#### 2.2.2.1 PWM Control Servo Motor Connection




The figure below is specifying the port for each SMLab iCrab’s merus legs.

Figure 7: SMLab iCrab’s Merus legs

The figure below is specifying the port for each SMLab iCrab walking leg.

Figure 8: SMLab iCrab’s Walking legs


### 2.2.3 Battery Connector & RGB Led

Figure 9: Battery connector & RGB led

The figure above showing Battery Connector and RGB Led. Battery connector is for battery to connect to provide power supply. The RBG led is SK6812MINI. It is a smart LD control circuit and light emitting circuit in one controller LED source. It able to display any color base on the combination of red , blue and green.

### 2.2.4 Switch


The figure below showing the switch .It is a latching switch. It able to cut of the battery supply.

Figure 10: Battery Switch


### 2.2.5 MT3608 step-up converter

MT3608 step up converter circuit. It able to convert lithium battery voltage ( 3.7v ) to 5v.

The figure below is showing the MT3608 step converter circuit.


Figure 11: MT3608 Step-up Converter circuit

The figure below is showing the schematic of MT3608 step up converter circuit

Figure 12: Schematic of MT3608 step up converter


### 2.2.5 Buzzer

The figur below showing the buzzer. It is a passive buzzer that able to have different tone with change the frequency of the PWM signal.

Figure 13: Buzzer

### 2.2.6 TP4056 module

TP4056 is a complete constant-current/constant-voltage linear charger for single cell lithium-ion batteries. It provide a usb type C port for us to charge the lithium battery. The figure below showing th TP4056 module.


Figure 14: TP4056 Module

### 2.2.7 Capacitor and resistor

The figure below showing capacitor and resistor

The C1 is an electrolytic capacitor is a capacitor that uses an oxide film made of aluminum, tantalum or other oxidizable metal as a dielectric. The parameter of C1 is 10v 470uF . The C2 and C3 is a ceramic capacitor where the ceramic material acts as the dielectric The paramter of C2 and C3 are 25v 22uF. In this case capacitor is to prevent voltage drip and stablize the voltage.

The resistor R1 and R2 is acting as a voltage divider for ESP32 to measure the voltage of Battery through ADC. The value of R1 and R2 are 10k and 2k . We have to use resistor because ESP32 have a 12 bit ADC which only able to measure 0 to 3.3v ( 0 – 4095 ) . We add resistor to limit the current and also the voltage in order not to burn the esp32. The figure below is showin capacitors and resistors.


Figure 15: Capacitor and resistor

# 2.3 Bom list

* iSEB Expansion Board 1200 0012 V1.0 with ESP32 Module x 1
* 18650 Battery x 2
* ESP32-DEVKIT-V1 x 1
* Crab chassis set x 1

# 3 Firmware

The iSEB Expansion Board 1200 0012 V1.0 is using ESP32 DevKit V1. The figure is showing the pinout of ESP32 DevKit V1.The microcontroller is esp-wroom-32 module.

Figure 16: Pinout of ESP32 DevKit V1

## 3.1 Specification of the ESP32 DevKit V1


Microcontroller: Tensilica 32-bit Single-/Dual-core CPU Xtensa LX6

* Operating Voltage: 3.3V
* Input Voltage: 7-12V
* Digital I/O Pins (DIO): 25
* Analog Input Pins (ADC): 6
* Analog Outputs Pins (DAC): 2
* UARTs: 3
* SPIs: 2
* I2Cs: 3
* Flash Memory: 4 MB
* SRAM: 520 KB
* Clock Speed: 240 Mhz
* Wi-Fi: IEEE 802.11 b/g/n/e/i:
  + Integrated TR switch, balun, LNA, power amplifier and matching network
  + WEP or WPA/WPA2 authentication, or open networks
* Dimensions: 51.5x29x5mm


## 3.2 Environment set up

We need to set up the environment to flash the binary to ESP32 DevKit V1.


* Install Arduino IDE is requried to install. ( Snapshot is base on Arduino IDE 2.2.0 )
* Add <https://raw.githubusercontent.com/espressif/arduino-esp32/gh-pages/package_esp32_index.json> to Board Managers and install ESP32 libary.
  + The figure below showing how to update board managers

Figure 17: File -> Preferences and click on the icon


* + The figure showing after adding the Boards Manager URLs

Figure 18: Adding board manager URLS


* + The figure below showing how to install ESP32 by Espressif Systems at Board Manager.

Figure 19: Install ESp32 by Espressif Systems at Board Managers


* + Install WS2812FX by Harm Aldick ( version 1.4.2 ) library.
  + The figure below showing how to install WS2812FX libary

Figure 20: Instal WS2812FX library

* The figure below showing how to update the upload setting

Figure 21: Upload setting

* Click upload button and the firmware will be flashed successfully if the snapshot below is seen.
* The figure below showing how to compile and upload the firmwrae

Figure 22: Compile and upload

* The environment set up is done if the binary able to flash to ESP32 DevKit V1


## 3.3 WiFi

### 3.3.1 How the WiFi Code works


* Firstly we need to include WiFi and WebServer library
  + #include <WiFi.h>
    - WiFi.h - esp32 Wifi support.
  + #include <WebServer.h>
    - WebServer.h - Dead simple web-server. Supports only one simultaneous client, knows how to handle GET and POST.
* Secondly we need to insert our ssid and password
  + const char\* ssid = "iSEB Crab";  // Enter SSID here
  + const char\* password = "12345678";  //Enter Password here
* Then we set our web server to port 80
  + WebServer server(80);
* We have to setup the WiFi in setup function
  + To start the Wi-Fi as an Access Point.
    - WiFi.softAP(ssid);/\* without password \*/
    - WiFi.softAP(ssid,password);/\* with password \*/
  + Function used to configure the IP as static (fixed) as well as the gateway and subnet.
    - WiFi.softAPConfig(local\_ip, gateway, subnet); /\* to add exception to server \*/
  + Set up handling of web page
    - server.on("/",handleIndex);
    - server.on("/editor", handleEditor);
    - server.on("/controller", handleController);
    - server.on("/zero", handleZero);
    - server.on("/setting",handleSetting);
    - server.on("/save", handleSave);
  + Enable the server
    - server.begin();
* We have to handle the user request in loop funtion
  + - server.handleClient();

### 3.3.2 WiFi server and control UI


* After flash succesfully, the iSEB Crab should be appear in the WiFi list. The figure below is showing the iSEB Crab is appeared in the WiFi list.

Figure 23: WiFi List


* The figure below showing how to access ISEB Crab through web broswer

Figure 24: Access ISEB Crab through web broswer


* The figure below is showing control page

Figure 25: Control Page

* The figure below is showing Motion Editor Page

Figure 26: Motion Editor Page

* The figue below is showing Zero Page


Figure 27: Zero Page

* The figure below is shwoing Setting page

Figure 28: setting page

## 3.4 Servo Motor

* The servo motor used in the iSEB Crab is TowerPro SG90 servo .
* The wire colors are Red = Battery(+) Brown = Battery(-) Orange = Signal
* The figure below show how the servo motor angle control by pwm
* Servo motor control with 50 Hz pulse width modulated (PWM) signal, which produces a pulse every 20ms.

Figure 29: How servo’s position controlled by PWM signal

### 3.4.1 How the Servo Motor Code works

#### 3.4.1.1 Setup

* We are using the LED Control library from ESP32 hal library to control servo motor.
* The LED control (LEDC) peripheral is primarly designed to control the intensity of LEDs, although it can also be used to generate PWM signals for other purposes. .
* For more details of the LEDC library can refer to the link
  + https://espressif-docs.readthedocs-hosted.com/projects/arduino-esp32/en/latest/api/ledc.html
* We able to generate PWM signals to control the servo motor.
* We have a motorInit funciton in the setup function to call the setup.
* We are calling funcition ledcSetupledc and ledcAttachPin in function motorInit.
* Function ledcSetupledc is used to setup the LEDC channel frequency and resolution.
  + uint32\_t ledcSetup(uint8\_t channel, uint32\_t freq, uint8\_t resolution\_bits);
    - channel select LEDC channel to config.
      * ESP32 have 16 channels
    - freq select frequency of pwm.
    - resolution\_bits select resolution for ledc channel.
      * range is 1-14 bits (1-20 bits for ESP32)
* Function ledcAttachPin is used to attach the pin to the LEDC channel.
  + void ledcAttachPin(uint8\_t pin, uint8\_t chan);
    - pin select GPIO pin.
    - chan select LEDC channel.
* The follow table is showing the GPIO vs Channel vs Connector in the example code

|  |  |  |  |
| --- | --- | --- | --- |
| **Walking/Merus** | **GPIO** | **Channel** | **Connector** |
| WALKING1 | 19 | 1 | CN15 |
| WALKING1 | 15 | 2 | CN9 |
| WALKING1 | 33 | 3 | CN7 |
| WALKING1 | 13 | 4 | CN1 |
| MERUS1 | 23 | 5 | CN16 |
| MERUS2 | 4 | 6 | CN10 |
| MERUS3 | 32 | 7 | CN8 |
| MERUS4 | 12 | 8 | CN2 |

Table 2: Position vs GPIO vs Channel vs Connector matrix

#### 3.4.1.2 Code of motorInit function

// use 12 bit precission for LEDC timer

#define LEDC\_TIMER\_12\_BIT  12

// use 50 Hz as a LEDC base frequency

#define LEDC\_BASE\_FREQ     50

#define WALKING\_1 0 /\* Chanel 0 \*/

#define WALKING\_2 1 /\* Chanel 1 \*/

#define WALKING\_3 2 /\* Chanel 2 \*/

#define WALKING\_4 3 /\* Chanel 3 \*/

#define MERUS\_1 4 /\* Chanel 4 \*/

#define MERUS\_2 5 /\* Chanel 5 \*/

#define MERUS\_3 6 /\* Chanel 6 \*/

#define MERUS\_4 7 /\* Chanel 7 \*/

void motorInit()

{

  // Setup timer

  ledcSetup(WALKING\_1, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(WALKING\_2, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(WALKING\_3, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(WALKING\_4, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(MERUS\_1, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(MERUS\_2, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(MERUS\_3, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  ledcSetup(MERUS\_4, LEDC\_BASE\_FREQ, LEDC\_TIMER\_12\_BIT);

  // Attach timer to a led pin

  ledcAttachPin(19, WALKING\_1);  /\* WALKING\_1 \*//\* CN15 \*//\* PIN 19\*/

  ledcAttachPin(15, WALKING\_2);  /\* WALKING\_2 \*//\* CN9  \*//\* PIN 15\*/

  ledcAttachPin(33, WALKING\_3);  /\* WALKING\_3 \*//\* CN7  \*//\* PIN 33\*/

  ledcAttachPin(13, WALKING\_4);  /\* WALKING\_4\*//\* CN1  \*//\* PIN 13\*/

  ledcAttachPin(23, MERUS\_1);  /\* MERUS\_1 \*//\* CN16 \*//\* PIN 23\*/

  ledcAttachPin( 4, MERUS\_2);  /\* MERUS\_2 \*//\* CN10 \*//\* PIN  4\*/

  ledcAttachPin(32, MERUS\_3);  /\* MERUS\_3 \*//\* CN8  \*//\* PIN 32\*/

  ledcAttachPin(12, MERUS\_4);  /\* MERUS\_4 \*//\* CN2  \*//\* PIN 12\*/

  delay(50);

}

* From the code above we have set up pwm channel 0 to 7 to 50hz frequeny with resolution 12 bit with function ledcSetup
* We have assign GPIO pin to the pwm channel accordingly with function ledcAttachPin.

#### 3.4.1.3 Update duty cycle during runtime

* ESP32 will output pwm signal after we configure the frequenc , resolutoin to the pwm channel and assign the GPIO pin to each pwm channel.
* We can call LEDCWrite to update the duty cycle of the particular pwm channel.
* By updating duty cycle we can control the positoin of servo motor mention chalter 3.4
* Functoin ledcWrite is used to set duty for the LEDC channel.
  + void ledcWrite(uint8\_t chan, uint32\_t duty);
    - chan select the LEDC channel for writing duty.
    - duty select duty to be set for selected channel.
* In the example code, we have set the resolution bit to 12 bit hence there are 4095 steps for the reoslution.
* By calculation we set 409 to acheive 1ms duty cycle and 819 to achieve 2ms duty cycle.
* However the example we set min to 50 min and maximum to 550 due to base on testing the servo motor only react between 50 and 550 ( will further investigate on this issue suspect is due to servo motor but yet to confirm with scope ).
* For the servo postion array such as Servo\_Prg\_X, the position is store as position therefore a positoin convert to duty cycle is needed.
* Function Set\_PWM\_to\_Servo is to convert the position to duty cycle and update to the pwm channel
  + void Set\_PWM\_to\_Servo(int iServo, int iValue)
    - iServo select the LEDC channel for writing duty.
    - Ivalue select the position to convert to duty tobe set for selected channel.

#### 3.4.1.4 Set\_PWM\_to\_Servo

/\* MOTOR CODE START \*/

void Set\_PWM\_to\_Servo(int iServo, int iValue)

{

  Serial.print(F("iServo: "));

  Serial.print(iServo);

  Serial.print(F(" iValue: "));

  Serial.println(iValue);

  // Read from EEPROM to fix zero error reading

  iValue = (iValue\*MAX/180.0)+MIN; /\* convertion to pwm value \*/

  double NewPWM = iValue + preferences.getDouble((String(iServo)).c\_str(),0);

  /\* 0 = zero degree 550 = 180 degree\*/

  ledcWrite(iServo,NewPWM);

}

* We have printed the input parameter iServo and iValue for debug purpose.
* We have do conversion for iValue from position to duty cycle
* We have done the zero error calibration but currently not in use the value will always be zero.
* We will udpate the pwm channel value with ledcWrite.